Information: Configuration: HAAS Turning

Information: Vendor: Haas Automation

Information: Posting intermediate data to 'E:\1001.nc'

Information: Total number of warnings: 3

Error: Failed to post process. See below for details.

...

Code page changed to '1252 (ANSI - Latin I)'

Start time: Wednesday, October 23, 2019 4:18:30 PM

Warning: function getProgramNameAsInt does not always return a value

Warning: function getProgramNameAsInt does not always return a value

Warning: function getProgramNameAsString does not always return a value

Code page changed to '20127 (US-ASCII)'

Post processor engine: 4.3.0 45264

Configuration path: C:\Users\cholland\AppData\Local\Autodesk\webdeploy\production\27887f06acbb684cb4cacf2fdbd563eef8f1b732\Applications\CAM360\Data\Posts\haas turning.cps

Include paths: C:\Users\cholland\AppData\Local\Autodesk\webdeploy\production\27887f06acbb684cb4cacf2fdbd563eef8f1b732\Applications\CAM360\Data\Posts

Configuration modification date: Wednesday, July 03, 2019 8:17:04 AM

Output path: E:\1001.nc

Checksum of intermediate NC data: 66dbd747a95a14a24bf3531d2fc68e14

Checksum of configuration: 46d30c306b79f11010f3359bc271e259

Vendor url: https://www.haascnc.com

Legal: Copyright (C) 2012-2018 by Autodesk, Inc.

Generated by: Fusion 360 CAM 2.0.6516

...

###############################################################################

Error: Turret number must be 0 (main turret), 101 (QCTP X-), 102 (QCTP X+, 103 (gang tooling X-), or 104 (gang tooling X+).

Error at line: 651

Error in operation: 'Profile Roughing1'

Failed while processing onSection() for record 375.

###############################################################################

Error: Failed to invoke function 'onSection'.

Error: Failed to invoke 'onSection' in the post configuration.

Error: Failed to execute configuration.

Stop time: Wednesday, October 23, 2019 4:18:30 PM

Post processing failed.